**To Use AC**

**AC uses sea water to cool the compressor, to enable operations you must 1st open the seacock located below the 3 drawer lockers prior to turning on the system.**

**When the compressor is working correctly you will see stream of water out of the starboard drain above waterline.**

**When leaving dock close the seacock to prevent drain down of sea water when healed over.**

**If the system is drained, or air gets in it the pump will not push water and the compressor will just cycle on and off.**

**To correct the problem, or to prime the system after being drained, disconnect the outflow tube and lower it below the pump till water flow in from the open sea cock. Then close seacock and reattach the outflow line.**