Onyx Outdoor July 27, 2019

1209 Franklin Avenue NE  
Sauk Rapids, MN  
56379

Fax (320)252-2160

Email: absolute@absoluteoutdoorinc.com

I would like to report the failure of one of my Onyx A/M|24 PDF.

The failure occurred when the charging head failed at what looks to be a pressure relief on the head prior to the inflation valve. The unit involved is approximately 2 – 3 years old and had never been activated but had had the yearly rearming process performed at the start of the season. The kits used were the Onyx kit 1352; k320. The head caries a set of numbers u9000 051316. It appears that the o-ring under the pressure relief (if that is what it is) failed and split.

As this is a life safety device and is not only a required boating equipment I am deeply concerned with the reliability of the line as well as the safety of those on board my sailboat, Even more so in that I bought 3 vests at the same time differing only in the colors (the failing one is blue).

I have retained the vest to allow your QC engineering to determine if this is a one off or a supplier problem.

Needless to say, until this issue is resolved I will be replacing the all onboard vests as a Captain of a vessel I could be held libel for loss of life due to your products failures.

I eagerly await a response to this event as well a recommendation for replacement PDFs that either you manufacture or view as strong safe competitor.

I am required to report this failure to the Annapolis Coast Guard and would like to be able to report favorably of your actions to insure the reliability of this product.

Dan Freedman

SV Full Sail

[dan@done-that.com](mailto:dan@done-that.com)

240-344-9964